Meeting with Kerttu 14.2.18

- installation of three video projections looping in a darkened room (black box)

- surround sound or sound coming from headphones

- a wind machine synced with the master video, starts when videos are black

Questions:

- Should there be a tricker starting the video?

- Should the installation be for one viewer at a time?

- What is the technical solution for the wind machine so that it wouldn’t make too much noise? Noice cancelling headphones? Wind machine in a nother room?

- How to fade the wind in/out

Solutions:

- Three Brightsigns, three projectors synced through Ethernet

- Ardruino controlling the wind machine